Material Safety Data Sheet
SECTION I - COMPANY IDENTIFICATION
PRODUCT: SUNISO 4GS REFRIGERATION OIL					CAT. NO.:	L317, L319, L322, L325

PACKED & DISTRIBUTED BY:						TELEPHONE NUMBERS:
Virginia KMP Corporation							Office:		1-(214) 330-7731
4100 Platinum Way								Emergency Only:	1-(800) 424-9300
Dallas, Texas 75237
SECTION II - HAZARDOUS INGREDIENTS
OSHA Hazardous Components (29 CFR 1910.1200)				EXPOSURE LIMITS: 8 HR. TWA
									OSHA PEL		ACGIH TLV

Mineral oil (CAS# 64742-52-5)							NE			5 mg/m3  (mist)
SECTION III - HAZARDS IDENTIFICATIONS
EMERGENCY OVERVIEW:	CAUTION!  Eye and skin irritant.  Harmful if swallowed.

POTENTIAL HEALTH EFFECTS:
	INHALATION:	Harmful if inhaled, but unlikely in normal use.
	EYE CONTACT:	Eye irritation develops immediately upon contact.
	SKIN CONTACT:	Causes skin irritation; may aggravate pre-existing skin disorders.
	INGESTION:	Irritates gastrointestinal tract.

	CHRONIC Effects:	None Established

	NOTE:

	CARCINOGENICITY: LISTED IN NTP?   No			IARC?   No			OSHA Regulated?   No
SECTION IV - FIRST AID MEASURES
INHALATION:	Remove victim to fresh air and, if needed, immediately begin artificial respiration.  Give oxygen if breathing is labored.  Get emergency medical help.  Contact a physician immediately.
EYE CONTACT:	Flush eyes with water for 15 minutes.  Get medical attention if symptoms develop and persist.
SKIN CONTACT:	Flush with water or soap and water for 15 minutes or until all traces have been removed.  Seek medical attention if symptoms develop and persist.
INGESTION:	Do NOT induce vomiting.  Rinse mouth out with water.  Get immediate medical attention.
SECTION V - FIRE FIGHTING MEASURES
FLASHPOINT (TEST METHOD):	302 F
FLAMMABLE LIMITS:		LOWER:	ND			UPPER:	ND
AUTOIGNITION TEMPERATURE:	ND

GENERAL HAZARD:	Combustible liquid, acrid smoke and irritating fumes.
FIRE FIGHTING INSTRUCTIONS:	Keep unnecessary people away; isolate area.  Firefighters should wear NIOSH approved, self contained breathing apparatus.  Approach fire from upwind side.  Avoid breathing smoke, fumes, mist, or vapors on the downwind side.

EXTINGUISHING MEDIA:	Dry powder, carbon dioxide (CO2), water fog or spray.
HAZARDOUS COMBUSTION PRODUCTS:	Smoke, carbon monoxide, carbon dioxide.
SECTION VI - ACCIDENTAL RELEASE MEASURES
LAND SPILL:	Emergency response coordinator must have mandated training.  Eliminate all ignition sources.  SMALL SPILLS: Pick up with absorbent materials and place in non-leaking containers; seal tightly for proper disposal or reuse.  LARGE SPILLS: Evacuate the hazard area of unprotected personnel.  Wear appropriate respirator and protective clothing.  Shut off source of leak if safe to do so.  Dike and contain.  Remove with vacuum trucks or pump to storage/salvage vessels.

WATER SPILL:	Floating water hazard.  Collect and place in chemical waste container.  Notify appropriate authorities.

Clean up leaks/spills immediately to prevent soil or water contamination.
SECTION VII - HANDLING AND STORAGE
HANDLING:	After handling this product, wash hands before eating, drinking, or smoking.  Avoid contact with skin, eyes, and clothing.  If contact occurs, remove contaminated clothing.  If needed, take first aid action shown in Section IV.  Launder contaminated clothing before reuse.

STORAGE:	Store away from oxidizers.  Store away from sources of ignition.

SECTION VIII - EXPOSURE CONTROLS/PERSONAL PROTECTION
ENGINEERING CONTROLS:	Local exhaust ventilation recommended.
PERSONAL PROTECTION:	Use gloves to prevent prolonged skin contact.
SECTION IX - PHYSICAL AND CHEMICAL PROPERTIES
VAPOR PRESSURE: Negligible					VAPOR DENSITY (Air=1): >5
SPECIFIC GRAVITY: 0.9						EVAPORATION RATE (N-BUTYL ACETATE=1): >1
SOLUBILITY IN WATER: Insoluble					VOC (G/L): 0
pH: NA								FREEZING POINT:
BOILING POINT: 260 C
APPEARANCE & ODOR: Light golden liquid, oil odor
SECTION X - STABILITY AND REACTIVITY
STABILITY:	Stable.
CONDITIONS TO AVOID:	Ignition sources.
MATERIALS TO AVOID:	Oxidizers.
HAZARDOUS DECOMPOSITION PRODUCTS:	Combustion:  Smoke, carbon monoxide, carbon dioxide.
HAZARDOUS POLYMERIZATION:	Will not occur.
SECTION XI - TOXICOLOGICAL INFORMATION
Mineral oil				LD50: 402 g/kg   (skin: mouse)
SECTION XII - ECOLOGICAL INFORMATION
Not available.
SECTION XIII - DISPOSAL CONSIDERATIONS
Dispose as hazardous waste.  Classification and documentation is required before disposal.  Follow all local, state and federal regulations.
SECTION XIV - TRANSPORTATION INFORMATION
PROPER SHIPPING NAME:	Not regulated.

HAZARD CLASS:		NA
IDENTIFICATION NUMBER:	NA
DOT Emergency Guide #:	171
Reportable Quantity (RQ):	NA
International:		NA
SECTION XV - REGULATORY INFORMATION
TSCA (Toxic Substance Control Act):	Components of this product are listed on the TSCA Inventory.
CERCLA (Comprehensive Environmental Response, Compensation and Liability Act):	Not listed.

SARA TITLE III (Superfund Amendments and Reauthorization Act):	None listed.

CALIFORNIA PROPOSITION 65:	WARNING: This product contains mineral oils, a chemical known to the State of California to cause cancer.
SECTION XVI - OTHER INFORMATION
State Right-to-Know Programs:	None

NFPA Ratings
	Health:		0
	Flammability:	0
	Reactivity:	0
HMIS Protective Equipment:	X   See your supervisor